Roll-a-Flex NBS spec

* **J.31 Liquid Applied Waterproof Roof Coatings**
* **- Brand Owner**
* M.R. Site Services Ltd, Unit 6,
* Worcester Trading Estate,
* Blackpole Road,
* Worcester.
* WR3 8HR.
* United Kingdom
* UK dialling code 0044
* Tel.01905 755055 Fax.01905 755053
* E-mail: [welding@mrsiteserivces.co.uk](mailto:welding@mrsiteserivces.co.uk)   
   Internet: [www.mrsiteservices.co.uk](http://www.mrsiteservices.co.uk/)
* **- Brand**
* Quantum Roll-a-Flex Sealing Systems
* **- Size**
* Various widths available, 150mm, or multiples of 1050mm
* **- Material**
* PMMA technology - Polymethylmethacrylate / Polyurathane
* BS476:Part3:2004 – EXT.F.AA
* **- German Standard**
* Test Method 1/prENV 1187; Classification B roof(t1)prEN 13501-5
* **- Fabrication**
* As per standard M.R. Site Services Ltd, drawings
* **- Usage** Roll-a-Flex sealing System comprises various certified products to
* create a versatile adhesive and water tight solution to sealing roofing
* details, adheres to virtually all materials and products
* **- Weight example**
* A 1000sq x 5mm thick area weighs approx. 3.65 kilos
* **- Width**
* Various widths available, 150mm, or multiples of 1050mm

**- Variations**

Suitable for all common roof constructions

Suitable for in service use in all climate zones

* Elastomeric and dynamic crack bridging
* Totally cold applied
* Exceptionally fast curing
* Can be applied at low temperatures (-5°c)